ANDEN AS80 - Replacement Canister for ANDEN Steam Humidifier Model: AS35 and AS35FP

Anden Steam Humidifiers are a grow room solution that helps you achieve ideal conditions through humidity control. As water in the canister boils and turns into steam, minerals are left behind. Minerals remaining in solution increase the conductivity of the water. Minerals also deposit onto the submerged portions of the electrodes rendering those areas ineffective. As this occurs, the level of water in the canister rises to expose uncoated electrode surface. 

· INCLUDES: (1) Replacement canister for ANDEN Humidifier Model: As35 and AS35FP
(1) new O-ring into groove in drain assembly. (O-ring is provided with Model AS80 canister.) Dampen O-ring with water before inserting canister. Do not use oil, grease, or any lubricant besides water
· Anden Humidifiers are designed with easy access for simple canister changes
· The Model AS80 typically works best when the Steam Humidifier is installed at 208 or 240 VAC . If the Steam Humidifier has a yellow Steam light in the first two weeks of running with a new canister, the Steam Humidifier is taking a long time to reach its nominal current; changing to the Model AS80LC canister will prevent this from happening in the future
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· Length/Depth (Inches): 19.75
· Width (Inches): 13
· Height (Inches): 14
· Weight (Pounds): 1.56
· Cubic Measurement: 2.080150463
· Shipping Length/Depth (Inches): 20
· Shipping Width (Inches): 13
· Shipping Height (Inches): 14
· Shipping Weight (Pounds): 2

